Andrew Giardina

Internetworking

CMPT 307N 112

January 28, 2020

Lab 2A

**Q1**. There are 12 available commands in EXEC mode on the Switch.

**Q2**. Hitting SPACE in the –MORE—tab shows much more data. Specifically, it shows all data regarding the next FastEthernet port. While the ENTER button just shows the next set of data one line at a time.

**Q3**. The Base Ethernet MAC Address is 0001.64D5.4455

**Q4**. The Show History command shows all of the commands you have currently entered in the CLI

**Q5**. It displays “enable password marist”

**Q6**. The “No Hostname” command simply resets the name to its default. So it’s Router once again.

Packet Tracer Screenshot for Parts A, B, C

